
Options ResourceUsage=yes UseNutmegFormat=no TopDesignName="H:\Research_Work\ADS_Sims\LTE_DL_Rx_prj\networks\LTE_DL_TX_EVM"
define LTE_SpecShaping ( _net6309  _net6304 ) 
parameters  Bandwidth=2  OversamplingOption=1  CyclicPrefix=0  IdleInterval=0.0  SpectrumShapingType=1  FilterType=0  Taps=19  FIRwithInterp=0  Alpha=0.22  WindowType=0  CyclicInterval=6 
_vAgilentEEsof_dHOF_nIfElse_lhofstars:SpectrumShaping  _net6309 _net6313 _net6311 _net6312 _net6314 _net6310 Condition=SpectrumShapingType 
_vAgilentEEsof_dSDF_nLTE_x5fSymWindow_lsdfltestars:Time_Windowing  _net6310 _net6311 Bandwidth=Bandwidth OversamplingOption=OversamplingOption CyclicPrefix=CyclicPrefix IdleInterval=IdleInterval WindowType=WindowType CyclicInterval=CyclicInterval 
_vAgilentEEsof_dSDF_nLTE_x5fSpectrumShaping_lsdfltestars:FIR_SpectShaping  _net6312 _net6313 Bandwidth=Bandwidth OversamplingOption=OversamplingOption FilterType=FilterType Taps=Taps FIRwithInterp=FIRwithInterp Alpha=Alpha IdleInterval=IdleInterval 
_vAgilentEEsof_dHOF_nBus_lhofstars:B1  _net6314 _net6304 BusWidth=1 
end LTE_SpecShaping
define LTE_DL_OFDM_Modulator ( _net383  _net376 ) 
parameters  Bandwidth=2  OversamplingOption=1 

Base_DFTSize=if (Bandwidth==0) then 128 elseif (Bandwidth==1) then 256 elseif (Bandwidth==2) then 512 elseif (Bandwidth==3) then 1024 elseif (Bandwidth==4) then 1536 else 2048 endif
NumOfRBs=if (Bandwidth==0) then 6 elseif (Bandwidth==1) then 15 elseif (Bandwidth==2) then 25 elseif (Bandwidth==3) then 50 elseif (Bandwidth==4) then 75 else 100 endif
UsedCarriers=12*NumOfRBs
_vAgilentEEsof_dHOF_nNop_lhofstars_poutput_x3d2_aBusSplit2:B14  _net385 _net386 _net387 
_vAgilentEEsof_dSDF_nAsyncDistributor_lsdfstars:A10  _net383 _net385 BlockSizes="Half_UsedCarriers1 Half_UsedCarriers2" 
_vAgilentEEsof_dSDF_nConstCx_lsdfstars:C10  _net382 Real=0.0 Imag=0.0 
_vAgilentEEsof_dHOF_nNop_lhofstars_pinput_x3d4_aBusMerge4:B16  _net377 _net387 _net382 _net386 _net381 
_vAgilentEEsof_dSDF_nGainCx_lsdfstars:G1  _net388 _net376 Gain=DFTSize 
_vAgilentEEsof_dSDF_nConstCx_lsdfstars:C11  _net377 Real=0.0 Imag=0.0 
_vAgilentEEsof_dSDF_nAsyncCommutator_lsdfstars:A9  _net381 _net373 BlockSizes="1 Half_UsedCarriers2 DFT_zeros Half_UsedCarriers1" 

DFTSize=Base_DFTSize*2^OversamplingOption
DFT_zeros=DFTSize-UsedCarriers-1
Half_UsedCarriers1=int (UsedCarriers/2)
Half_UsedCarriers2=int (UsedCarriers/2)
_vAgilentEEsof_dSDF_nLTE_x5fFFT_lsdfltestars:L2  _net373 _net388 InputSize=DFTSize FFTSize=DFTSize Direction=0 
end LTE_DL_OFDM_Modulator
define LTE_DL_OFDM_Demodulator ( _net115  _net121 ) 
parameters  Bandwidth=2  OversamplingOption=1 

Base_DFTSize=if (Bandwidth==0) then 128 elseif (Bandwidth==1) then 256 elseif (Bandwidth==2) then 512 elseif (Bandwidth==3) then 1024 elseif (Bandwidth==4) then 1536 else 2048 endif
NumOfRBs=if (Bandwidth==0) then 6 elseif (Bandwidth==1) then 15 elseif (Bandwidth==2) then 25 elseif (Bandwidth==3) then 50 elseif (Bandwidth==4) then 75 else 100 endif
UsedCarriers=12*NumOfRBs
_vAgilentEEsof_dSDF_nAsyncDistributor_lsdfstars:A7  _net127 _net128 BlockSizes="1 Half_UsedCarriers1 DFT_zeros Half_UsedCarriers2" 
_vAgilentEEsof_dHOF_nNop_lhofstars_poutput_x3d4_aBusSplit4:B9  _net128 _net123 _net124 _net125 _net126 
_vAgilentEEsof_dSDF_nAsyncCommutator_lsdfstars:A8  _net120 _net121 BlockSizes="Half_UsedCarriers1 Half_UsedCarriers2" 
_vAgilentEEsof_dHOF_nNop_lhofstars_pinput_x3d2_aBusMerge2:B10  _net126 _net124 _net120 
_vAgilentEEsof_dSDF_nLTE_x5fFFT_lsdfltestars:FFT  _net115 _net127 InputSize=DFTSize FFTSize=DFTSize Direction=1 

DFTSize=Base_DFTSize*2^OversamplingOption
DFT_zeros=DFTSize-UsedCarriers-1
Half_UsedCarriers1=int(UsedCarriers/2)
Half_UsedCarriers2=int(UsedCarriers/2)
end LTE_DL_OFDM_Demodulator
define QAM_Demod ( _net96  _net93  _net91 ) 
parameters  RIn=DefaultRIn  ROut=DefaultROut  RTemp=DefaultRTemp  RefFreq=1000000  Sensitivity=1.0  Phase=0.0  GainImbalance=0.0  PhaseImbalance=0.0 
_vAgilentEEsof_dTSDF_n_x5fQAM_x5fDemod_ltsdfstars:Q1  _net96 _net97 _net98 RIn=RIn ROut=ROut RTemp=-273.15 RefFreq=RefFreq Sensitivity=Sensitivity Phase=Phase GainImbalance=GainImbalance PhaseImbalance=PhaseImbalance 
R:R1  _net96 0 R=RIn Temp=-273.15 
R:R2  _net97 _net93 R=ROut Temp=RTemp 
R:R3  _net98 _net91 R=ROut Temp=RTemp 
end QAM_Demod
define RF_Modulator ( _net401  _net403  _net385 ) 
parameters  ROut=DefaultROut  RTemp=DefaultRTemp  FCarrier=1900 MHz  Power=0.01 W  VRef=1 V  SamplingRate=25e3  MirrorSpectrum=0  GainImbalance=0.0  PhaseImbalance=0.0  I_OriginOffset=0.0  Q_OriginOffset=0.0  IQ_Rotation=0.0 
_vAgilentEEsof_dSDF_nGain_lsdfstars:G5  _net403 _net400 Gain=Q_Gain 
_vAgilentEEsof_dTSDF_nFloatToTimed_ltsdfstars:F2  _net400 _net398 TStep=TStep 
_vAgilentEEsof_dSDF_nGain_lsdfstars:G6  _net401 _net396 Gain=I_Gain 
_vAgilentEEsof_dTSDF_nFloatToTimed_ltsdfstars:F1  _net396 _net394 TStep=TStep 
_vAgilentEEsof_dTSDF_n_x5fQAM_x5fMod_ltsdfstars:Q1  _net394 _net398 _net392 RIn=50.0 Ohm ROut=ROut Ohm RTemp=-273.15 FCarrier=FCarrier Hz Power=Power W VRef=4*VRef Phase=0 GainImbalance=GainImbalance PhaseImbalance=PhaseImbalance 
_vAgilentEEsof_dTSDF_n_x5fPhaseShiftRF_ltsdfstars:P1  _net392 _net389 RIn=ROut Ohm ROut=ROut Ohm RTemp=-273.15 PhaseShift=IQ_Rotation 
_vAgilentEEsof_dTSDF_nConstTimed_ltsdfstars:C3  _net387 TStep=TStep FCarrier=FCarrier Hz Value=Offset 
R:R2  _net402 _net385 R=ROut Temp=RTemp 

I_Gain=1
Q_Gain=if ( MirrorSpectrum == 0 ) then I_Gain else ( -I_Gain ) endif
Offset=( I_OriginOffset + j * Q_OriginOffset ) * sqrt( 2 * ROut * Power ) / 100
TStep=1 / SamplingRate
_vAgilentEEsof_dTSDF_n_x5fSummerRF_ltsdfstars:S1  _net387 _net389 _net402 RIn=ROut Ohm ROut=ROut Ohm RTemp=-273.15 FcOut=2 
end RF_Modulator
define LTE_DL_Src ( UE1  UE2  UE3  UE4  UE5  UE6  _net7702  frm_TD ) 
parameters  FrameMode=0  TDD_Config=0  Bandwidth=2  OversamplingOption=1  CyclicPrefix=0  CellID_Sector=0  CellID_Group=0  SymPerSub_PDCCH={ 3, 3, 3, 3, 3, 3, 3, 3, 3, 3 }  PHICH_Duration=0  PHICH_Ng=0  UE1_PRB_Bitmap={ 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1}  UE2_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE3_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE4_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE5_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE6_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  IdleInterval=0.0  SpectrumShapingType=1  FilterType=0  Taps=19  FIRwithInterp=0  Alpha=0.22  WindowType=0  CyclicInterval=6  PDCCH_Factor=1.0  PCFICH_Factor=1.0  PHICH_Factor=1.0  PSCH_Factor=1.077632  SSCH_Factor=1.077632  BCH_Factor=1.0  RS_Factor=1.0  UEs_Data_Factor={ 1.0, 1.0, 1.0, 1.0, 1.0, 1.0} 
_vAgilentEEsof_dSDF_nWaveForm_lsdfstars:W1  _net7736 Value="1 1 1 0 1 0 0 1 0 0 1 0 0 1 0 0 1 0 0 1 0 0 1 0" ControlSimulation=0 Periodic=1 Period=0 
_vAgilentEEsof_dSDF_nLTE_x5fPHICH_x5fModulator_lsdfltestars:PHICH_Modulator  _net7736 _net7730 Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix PHICH_Ng=PHICH_Ng FrameMode=FrameMode TDD_Config=TDD_Config CellID_Sector=CellID_Sector CellID_Group=CellID_Group SymPerSub_PDCCH=SymPerSub_PDCCH 
_vAgilentEEsof_dSDF_nLTE_x5fPHICH_x5fLayerMapper_lsdfltestars:PHICH_LayerMapper  _net7730 PHICH Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix NumOfLayers=1 PHICH_Ng=PHICH_Ng FrameMode=FrameMode TDD_Config=TDD_Config CellID_Sector=CellID_Sector CellID_Group=CellID_Group SymPerSub_PDCCH=SymPerSub_PDCCH 
LTE_SpecShaping:SpectrumShaping  _net7701 _net7702 Bandwidth=Bandwidth OversamplingOption=OversamplingOption CyclicPrefix=CyclicPrefix IdleInterval=IdleInterval SpectrumShapingType=SpectrumShapingType FilterType=FilterType Taps=Taps FIRwithInterp=FIRwithInterp Alpha=Alpha WindowType=WindowType CyclicInterval=CyclicInterval 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fMuxOFDMSym_lsdfltestars:BS_MuxOFDMSym  UE1 UE2 UE3 UE4 UE5 UE6 PSS SSS PBCH PDCCH PCFICH PHICH RS _net7699 frm_TD FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Group UE1_PRB_Bitmap=UE1_PRB_Bitmap UE2_PRB_Bitmap=UE2_PRB_Bitmap UE3_PRB_Bitmap=UE3_PRB_Bitmap UE4_PRB_Bitmap=UE4_PRB_Bitmap UE5_PRB_Bitmap=UE5_PRB_Bitmap UE6_PRB_Bitmap=UE6_PRB_Bitmap SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PHICH_Duration=PHICH_Duration PSCH_Factor=PSCH_Factor SSCH_Factor=SSCH_Factor BCH_Factor=BCH_Factor PDCCH_Factor=PDCCH_Factor PCFICH_Factor=PCFICH_Factor PHICH_Factor=PHICH_Factor RS_Factor=RS_Factor UEs_Data_Factor=UEs_Data_Factor 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:CFI  _net7670 DataPattern=1 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:PBCH_Mapper  _net7668 PBCH MappingType=0 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:PCFICH_Mapper  _net7670 PCFICH MappingType=0 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:DCI  _net7653 DataPattern=1 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:PDCCH_Mapper  _net7653 PDCCH MappingType=0 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:BCH  _net7668 DataPattern=1 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fPilot_lsdfltestars:ReferenceSymbol  RS Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Group NumOfTxAnt=1 Solution=0 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fMuxFrame_lsdfltestars:FrameLMultiplexer  _net7604 _net7701 Bandwidth=Bandwidth OversamplingOption=PreOversamp IdleInterval=IdleInterval 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fMuxSlot_lsdfltestars:SlotMultiplexer  _net7600 _net7604 Bandwidth=Bandwidth OversamplingOption=PreOversamp CyclicPrefix=CyclicPrefix 
LTE_DL_OFDM_Modulator:OFDM_Modulator  _net7699 _net7600 Bandwidth=Bandwidth OversamplingOption=PreOversamp 
_vAgilentEEsof_dSDF_nLTE_x5fSSCH_lsdfltestars:SSS  SSS CellID_Sector=CellID_Sector CellID_Group=CellID_Group 
_vAgilentEEsof_dSDF_nLTE_x5fPSCH_lsdfltestars:PSS  PSS CellID_Sector=CellID_Sector 

PreOversamp=if(FIRwithInterp) then 0 else OversamplingOption endif
end LTE_DL_Src
define LTE_DL_EVM ( _net68 ) 
parameters  RIn=50 Ohm  RTemp=- 273.15  RefFreq=2500 MHz  Sensitivity=1  Phase=0.0  GainImbalance=0.0  PhaseImbalance=0.0  FrameMode=0  TDD_Config=0  Bandwidth=2  OversamplingOption=1  CyclicPrefix=0  CellID_Sector=0  CellID_Group=0  SymPerSub_PDCCH={ 3, 3, 3, 3, 3, 3, 3, 3, 3, 3 }  PHICH_Duration=0  PHICH_Ng=0  UE1_PRB_Bitmap={ 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1}  UE2_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE3_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE4_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE5_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE6_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  PowerBoosting={0.0, 0.0, 0.0, 0.0, 0.0, 0.0}  MappingType={ 0, 0, 0, 0, 0, 0 }  PreDownsampling=0  IdleInterval=0.0  PDCCH_Factor=1.0  PCFICH_Factor=1.0  PHICH_Factor=1.0  PSCH_Factor=1.077632  SSCH_Factor=1.077632  BCH_Factor=1.0  RS_Factor=1.0  FramesToAverage=10  DisplayOption=0  MeasurementOption=0 

Post_Oversamp=if(PreDownsampling) then 0 else OversamplingOption endif
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fEVM_x5fSink_lsdflte_x5fmeasurements:UE6  UE6_Data _net263 _net264 _net265 _net266 _net267 _net268 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PRB_Bitmap=UE6_PRB_Bitmap FramesToAverage=FramesToAverage MappingType=MappingType[6] DisplayOption=DisplayOption MeasurementOption=MeasurementOption 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fEVM_x5fSink_lsdflte_x5fmeasurements:UE1  UE1_Data PSCH SSCH BCH PDCCH PCFICH PHICH FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PRB_Bitmap=UE1_PRB_Bitmap FramesToAverage=FramesToAverage MappingType=MappingType[1] DisplayOption=DisplayOption MeasurementOption=MeasurementOption 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fEVM_x5fSink_lsdflte_x5fmeasurements:UE2  UE2_Data _net249 _net250 _net251 _net252 _net253 _net254 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PRB_Bitmap=UE2_PRB_Bitmap FramesToAverage=FramesToAverage MappingType=MappingType[2] DisplayOption=DisplayOption MeasurementOption=MeasurementOption 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fEVM_x5fSink_lsdflte_x5fmeasurements:UE3  UE3_Data _net242 _net243 _net244 _net245 _net246 _net247 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PRB_Bitmap=UE3_PRB_Bitmap FramesToAverage=FramesToAverage MappingType=MappingType[3] DisplayOption=DisplayOption MeasurementOption=MeasurementOption 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fEVM_x5fSink_lsdflte_x5fmeasurements:UE4  UE4_Data _net235 _net236 _net237 _net238 _net239 _net240 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PRB_Bitmap=UE4_PRB_Bitmap FramesToAverage=FramesToAverage MappingType=MappingType[4] DisplayOption=DisplayOption MeasurementOption=MeasurementOption 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fEVM_x5fSink_lsdflte_x5fmeasurements:UE5  UE5_Data _net228 _net229 _net230 _net231 _net232 _net233 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PRB_Bitmap=UE5_PRB_Bitmap FramesToAverage=FramesToAverage MappingType=MappingType[5] DisplayOption=DisplayOption MeasurementOption=MeasurementOption 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fTimeFreqSync_lsdfltestars:Timing_and_Frequency_Sync  _net128 _net125 _net126 _net127 FrameMode=FrameMode Bandwidth=Bandwidth OversamplingOption=OversamplingOption CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector IdleInterval=IdleInterval 
_vAgilentEEsof_dSDF_nAsyncCommutator_lsdfstars:A9  _net97 _net98 BlockSizes="1 31 1 31" 
_vAgilentEEsof_dSDF_nAsyncDistributor_lsdfstars:A10  _net105 _net100 BlockSizes="5 31 31 5" 
_vAgilentEEsof_dSDF_nLTE_x5fPSCH_lsdfltestars:L1  _net105 CellID_Sector=CellID_Sector 
_vAgilentEEsof_dHOF_nNop_lhofstars_poutput_x3d4_aBusSplit4:B14  _net100 _net101 _net119 _net120 _net104 
_vAgilentEEsof_dSDF_nLTE_x5fFFT_lsdfltestars:L2  _net98 _net125 InputSize=64 FFTSize=64 Direction=0 
_vAgilentEEsof_dHOF_nNop_lhofstars_pinput_x3d4_aBusMerge4:B16  _net123 _net120 _net18 _net119 _net97 
LTE_DL_OFDM_Demodulator:OFDM_Demodulator  _net114 _net79 Bandwidth=Bandwidth OversamplingOption=Post_Oversamp 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fDemuxSlot_lsdfltestars:Slot_Demultiplexer  _net113 _net114 Bandwidth=Bandwidth OversamplingOption=Post_Oversamp CyclicPrefix=CyclicPrefix 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fDemuxFrame_lsdfltestars:Freq_Compensator  _net110 _net126 _net127 _net113 Bandwidth=Bandwidth OversamplingOption=OversamplingOption IdleInterval=IdleInterval PreDownsampling=PreDownsampling 
_vAgilentEEsof_dSDF_nMpyCx_lsdfstars_pinput_x3d2_aMpyCx2:Equalizer  _net111 _net118 UE 
_vAgilentEEsof_dHOF_nFork_lhofstars_poutput_x3d2_aFork2:F2  _net79 _net111 _net115 
_vAgilentEEsof_dHOF_nFork_lhofstars_poutput_x3d2_aFork2:F1  _net20 _net110 _net128 
QAM_Demod:Demodulator  _net68 _net22 _net21 RIn=RIn ROut=DefaultROut RTemp=RTemp RefFreq=RefFreq Sensitivity=Sensitivity Phase=Phase GainImbalance=GainImbalance PhaseImbalance=PhaseImbalance 

UE1_factor=10^(PowerBoosting[1]/10)
UE2_factor=10^(PowerBoosting[2]/10)
UE3_factor=10^(PowerBoosting[3]/10)
UE4_factor=10^(PowerBoosting[4]/10)
UE5_factor=10^(PowerBoosting[5]/10)
UE6_factor=10^(PowerBoosting[6]/10)
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fPilot_lsdfltestars:DL_Pilot_Gen  _net122 Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Group NumOfTxAnt=1 Solution=0 
_vAgilentEEsof_dSDF_nMathCx_lsdfomnistars:M3  _net121 _net118 Type=7 
_vAgilentEEsof_dTSDF_nTimedIQToCx_ltsdfstars:T1  _net22 _net21 _net20 
_vAgilentEEsof_dSDF_nConstCx_lsdfstars:C11  _net123 Real=0.0 Imag=0.0 
_vAgilentEEsof_dSDF_nConstCx_lsdfstars:C12  _net18 Real=0.0 Imag=0.0 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fChEstimator_lsdfltestars:Channel_Est_and_Interp  _net115 _net122 _net121 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Group 
_vAgilentEEsof_dSDF_nLTE_x5fDL_x5fDemuxOFDMSym_lsdfltestars:OFDMSym_Demultiplexer  UE UE1_Data UE2_Data UE3_Data UE4_Data UE5_Data UE6_Data PSCH SSCH BCH PDCCH PCFICH PHICH _net14 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Group UE1_PRB_Bitmap=UE1_PRB_Bitmap UE2_PRB_Bitmap=UE2_PRB_Bitmap UE3_PRB_Bitmap=UE3_PRB_Bitmap UE4_PRB_Bitmap=UE4_PRB_Bitmap UE5_PRB_Bitmap=UE5_PRB_Bitmap UE6_PRB_Bitmap=UE6_PRB_Bitmap SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Ng=PHICH_Ng PHICH_Duration=PHICH_Duration PSCH_Factor=PSCH_Factor SSCH_Factor=SSCH_Factor BCH_Factor=BCH_Factor PDCCH_Factor=PDCCH_Factor PCFICH_Factor=PCFICH_Factor PHICH_Factor=PHICH_Factor RS_Factor=RS_Factor UEs_Data_Factor={UE1_factor,UE2_factor,UE3_factor,UE4_factor,UE5_factor,UE6_factor} 
end LTE_DL_EVM
define SpectrumAnalyzerResBW ( _net51 ) 
parameters  Plot=0  RLoad=DefaultRLoad  RTemp=DefaultRTemp  Start=DefaultTimeStart  Stop=DefaultTimeStop  Window=0  ResBW=30 kHz  NumSegments=0  SegmentTime=1.0 msec 
R:R1  _net51 0 R=RLoad Temp=RTemp 
_vAgilentEEsof_dTSDF_n_x5fSpectrumAnalyzerResBW_ltsdfsinks:S1  _net51 Plot=Plot RLoad=RLoad RTemp=RTemp Start=Start Stop=Stop Window=Window ResBW=ResBW NumSegments=NumSegments SegmentTime=SegmentTime 
end SpectrumAnalyzerResBW
define LTE_DL_Src_RF ( _net245  _net246  _net247  _net248  _net249  _net250  _net255  _net251  _net252 ) 
parameters  ROut=50 Ohm  RTemp=- 273.15  FCarrier=2500 MHz  Power= 0.01 W   MirrorSpectrum=0  GainImbalance=0.0  PhaseImbalance=0.0  I_OriginOffset=0.0  Q_OriginOffset=0.0  IQ_Rotation=0.0  FrameMode=0  TDD_Config=0  Bandwidth=2  OversamplingOption=1  CyclicPrefix=0  CellID_Sector=0  CellID_Group=0  SymPerSub_PDCCH={ 3, 3, 3, 3, 3, 3, 3, 3, 3, 3 }  PHICH_Duration=0  PHICH_Ng=0  UE1_PRB_Bitmap={ 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1}  UE2_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE3_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE4_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE5_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  UE6_PRB_Bitmap={ 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0}  PowerBoosting={0.0, 0.0, 0.0, 0.0, 0.0, 0.0}  IdleInterval=0.0  SpectrumShapingType=1  FilterType=0  Taps=19  FIRwithInterp=0  Alpha=0.22  WindowType=0  CyclicInterval=6  PDCCH_Factor=1.0  PCFICH_Factor=1.0  PHICH_Factor=1.0  PSCH_Factor=1.077632  SSCH_Factor=1.077632  BCH_Factor=1.0  RS_Factor=1.0 
RF_Modulator:RF_Modulator  _net253 _net254 _net255 ROut=ROut RTemp=RTemp FCarrier=FCarrier Power=Power VRef=1 V SamplingRate=SamplingRate MirrorSpectrum=MirrorSpectrum GainImbalance=GainImbalance dB PhaseImbalance=PhaseImbalance I_OriginOffset=I_OriginOffset Q_OriginOffset=Q_OriginOffset IQ_Rotation=IQ_Rotation 
LTE_DL_Src:Downlink_Multiple_UEs_Source  _net245 _net246 _net247 _net248 _net249 _net250 _net251 _net252 FrameMode=FrameMode TDD_Config=TDD_Config Bandwidth=Bandwidth OversamplingOption=OversamplingOption CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Group SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Duration=PHICH_Duration PHICH_Ng=PHICH_Ng UE1_PRB_Bitmap=UE1_PRB_Bitmap UE2_PRB_Bitmap=UE2_PRB_Bitmap UE3_PRB_Bitmap=UE3_PRB_Bitmap UE4_PRB_Bitmap=UE4_PRB_Bitmap UE5_PRB_Bitmap=UE5_PRB_Bitmap UE6_PRB_Bitmap=UE6_PRB_Bitmap IdleInterval=IdleInterval SpectrumShapingType=SpectrumShapingType FilterType=FilterType Taps=Taps FIRwithInterp=FIRwithInterp Alpha=Alpha WindowType=WindowType CyclicInterval=CyclicInterval PDCCH_Factor=PDCCH_Factor PCFICH_Factor=PCFICH_Factor PHICH_Factor=PHICH_Factor PSCH_Factor=PSCH_Factor SSCH_Factor=SSCH_Factor BCH_Factor=BCH_Factor RS_Factor=RS_Factor UEs_Data_Factor={ UE1_factor, UE2_factor, UE3_factor, UE4_factor, UE5_factor, UE6_factor} 

UE1_factor=10^(PowerBoosting[1]/20)
UE2_factor=10^(PowerBoosting[2]/20)
UE3_factor=10^(PowerBoosting[3]/20)
UE4_factor=10^(PowerBoosting[4]/20)
UE5_factor=10^(PowerBoosting[5]/20)
UE6_factor=10^(PowerBoosting[6]/20)
_vAgilentEEsof_dSDF_nCxToRect_lsdfstars:C1  _net251 _net253 _net254 

SamplingFreq=if (0==Bandwidth) then 1.92 MHz elseif (1==Bandwidth) then 3.84 MHz elseif (2==Bandwidth) then 7.68 MHz else SamplingFreq1 endif
SamplingFreq1=if (3==Bandwidth) then 15.36 MHz elseif (4==Bandwidth) then 23.04 MHz else 30.72 MHz endif
SamplingRate=SamplingFreq*2^OversamplingOption
end LTE_DL_Src_RF

OversamplingOption=1
FCarrier=2500 MHz
Bandwidth=5
CP=if (CyclicPrefix= 0 ) then 1/14 else 1/4 endif
CyclicPrefix=0
UE1_MappingType=0
SymPerSub_PDCCH={ 3, 3, 3, 3, 3, 3, 3, 3, 3, 3 }
PRB_Bitmap1=if (3==Bandwidth) then {1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1} elseif(4==Bandwidth) then {1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1} elseif (5==Bandwidth) then {1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1} elseif (0==Bandwidth) then {1,1,1,1,1,1} elseif (1==Bandwidth) then {1,1,1,1,1,1,1,1,1,1,1,1,1,1,1} else {1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1} endif
PRB_Bitmap2=if (3==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif(4==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (5==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (0==Bandwidth) then {0,0,0,0,0,0} elseif (1==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} else {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} endif
PRB_Bitmap3=if (3==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif(4==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (5==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (0==Bandwidth) then {0,0,0,0,0,0} elseif (1==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} else {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} endif
PRB_Bitmap4=if (3==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif(4==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (5==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (0==Bandwidth) then {0,0,0,0,0,0} elseif (1==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} else {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} endif
PRB_Bitmap5=if (3==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif(4==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (5==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (0==Bandwidth) then {0,0,0,0,0,0} elseif (1==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} else {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} endif
PRB_Bitmap6=if (3==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif(4==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (5==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} elseif (0==Bandwidth) then {0,0,0,0,0,0} elseif (1==Bandwidth) then {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} else {0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0} endif
UE1_Size=62436
UEBitsPerFrame=Rate*UE1_Size
CellID_Sector=0
CellID_Group=0
LTE_DL_EVM:L2  _net2789 RIn=50 Ohm RTemp=- 273.15 RefFreq=FCarrier Sensitivity=1 Phase=0.0 GainImbalance=0.0 PhaseImbalance=0.0 FrameMode=0 TDD_Config=0 Bandwidth=Bandwidth OversamplingOption=OversamplingOption CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Sector SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Duration=0 PHICH_Ng=0 UE1_PRB_Bitmap=PRB_Bitmap1 UE2_PRB_Bitmap=PRB_Bitmap2 UE3_PRB_Bitmap=PRB_Bitmap3 UE4_PRB_Bitmap=PRB_Bitmap4 UE5_PRB_Bitmap=PRB_Bitmap5 UE6_PRB_Bitmap=PRB_Bitmap6 PowerBoosting={0.0, 0.0, 0.0, 0.0, 0.0, 0.0} MappingType={ UE1_MappingType,1,1,0, 0, 0} PreDownsampling=0 IdleInterval=0.0 sec PDCCH_Factor=1.0 PCFICH_Factor=1.0 PHICH_Factor=1.0 PSCH_Factor=1 SSCH_Factor=1 BCH_Factor=1.0 RS_Factor=1.0 FramesToAverage=20 DisplayOption=2 MeasurementOption=0 
SpectrumAnalyzerResBW:RF_Spectrum  _net2789 Plot=0 RLoad=DefaultRLoad RTemp=DefaultRTemp Start=DefaultTimeStart Stop=DefaultTimeStop Window=6 ResBW=15 kHz NumSegments=10 SegmentTime=1.0 msec 
LTE_DL_Src_RF:DL_Src_RF  UE1 UE2 UE3 UE4 UE5 UE6 _net2789 _net2751 _net2752 ROut=50 Ohm RTemp=- 273.15 FCarrier=FCarrier Power=dbmtow(SignalPower) MirrorSpectrum=0 GainImbalance=0 PhaseImbalance=0.0 I_OriginOffset=0.0 Q_OriginOffset=0.0 IQ_Rotation=0.0 FrameMode=0 TDD_Config=0 Bandwidth=Bandwidth OversamplingOption=OversamplingOption CyclicPrefix=CyclicPrefix CellID_Sector=CellID_Sector CellID_Group=CellID_Group SymPerSub_PDCCH=SymPerSub_PDCCH PHICH_Duration=0 PHICH_Ng=0 UE1_PRB_Bitmap=PRB_Bitmap1 UE2_PRB_Bitmap=PRB_Bitmap2 UE3_PRB_Bitmap=PRB_Bitmap3 UE4_PRB_Bitmap=PRB_Bitmap4 UE5_PRB_Bitmap=PRB_Bitmap5 UE6_PRB_Bitmap=PRB_Bitmap6 PowerBoosting={0.0, 0.0, 0.0, 0.0, 0.0, 0.0} IdleInterval=0.0 sec SpectrumShapingType=0 FilterType=0 Taps=19 FIRwithInterp=0 Alpha=0.22 WindowType=0 CyclicInterval=16 PDCCH_Factor=1.0 PCFICH_Factor=1.0 PHICH_Factor=1.0 PSCH_Factor=1.0 SSCH_Factor=1.0 BCH_Factor=1.0 RS_Factor=1.0 
DefaultNumericStart=0
DefaultNumericStop=100
DefaultTimeStart=0 usec
DefaultTimeStop=100 usec
DefaultSeed=1234567
DefaultRIn=50 Ohm
DefaultROut=50 Ohm
DefaultRLoad=1.0e18 Ohm
DefaultRTemp=-273.15
__DefaultPartition=1
__SimulationID=0
_vAgilentEEsof_dTSDF_nDF_ltsdf:DF DefaultTimeUnit=3 DefaultSeed=if (DefaultSeed==0) then 0 else (DefaultSeed+__SimulationID) endif DefaultPartition=__DefaultPartition SchedulerType=1 DeadlockManager=0 CktCosimInputs=0 OutputPlan="DF_Output" 
OutputPlan:DF_Output \
      Type="Output" \
      UseSavedEquationNestLevel=yes \
      SavedEquationNestLevel=2


SignalPower=10
Rate=if(0==UE1_MappingType) then 2 elseif(1==UE1_MappingType) then 4 else 6 endif
UEOccupiedTime=0.01*11/14
DataRate=UEBitsPerFrame*(1+CP)/UEOccupiedTime
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:D1  _net2713 DataPattern=1 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:Mapper1  _net2713 UE1 MappingType=UE1_MappingType 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:Mapper5  _net2676 UE5 MappingType=0 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:Mapper4  _net2674 UE4 MappingType=0 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:Mapper3  _net2672 UE3 MappingType=1 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:Mapper2  _net2670 UE2 MappingType=1 
_vAgilentEEsof_dSDF_nLTE_x5fMapper_lsdfltestars:Mapper6  _net2668 UE6 MappingType=0 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:D2  _net2670 DataPattern=1 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:D3  _net2672 DataPattern=0 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:D4  _net2674 DataPattern=1 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:D5  _net2676 DataPattern=1 
_vAgilentEEsof_dSDF_nDataPattern_lsdfdspstars:D6  _net2668 DataPattern=1 
