// varactor test circuit
simulator lang=spectre
include "varactor_q.scs" section=moscap
Vt (n 0) vsource mag=1
Xv (n 0) varactor
capacitanceInF ac freq=1/(2*M_PI) start=-2 stop=2 dev=Vt param=dc
save Xv:1
